PURGENVENT Model 7900AAV

2.1 AIR VENTING VALVES

* + 1. Series: PURGEnVENT as manufactured by AGF Manufacturing, Inc.

Product: M7900AAV Automatically Vent Air from the System. Automatic Air Venting Valve is a 1 inch (25 mm) ball valve, strainer, air vent, and purge assembly.

Standard: UL's "Product iQ" listing or "Approval Guide," published by FM Global, listing. NFPA 13, 13R, 13D (as applicable).

Pressure Rating: 300 psig (2070 kPa), 175 psi (1205 kPa) for air vent.

Body Material: Forged brass body.

Components: Integrated ball valve, stainless steel strainer, purge valve with hose connection (Field adjustable), thread cap with lanyard, automatic air vent.

Inlet Size: 1 inch NPT.

Outlet Size: 3/4 inch (19 mm) NPT.

\*\* NOTE TO SPECIFIER \*\* Delete product not required.

Optional Water Collection Accessories:

Product: Model 7920AI. Water Collection Assembly with Audible Alarm.

Product: Model 7925VI. Water Collection Assembly with Visual Indicator.