PURGENVENT Model 7950ILV

2.1 SPRINKLER SPECIALTY PIPE FITTINGS

* + - * 1. Main Line Air Vent:

Product: M7950ILV In-Line Automatic Air Venting Valve. The separation chamber and air scoop is designed to force a separation of air from the water as the system fills.

Standard: UL's "Fire Protection Equipment Directory" listing or "Approval Guide," published by FM Global, listing. NFPA 13, 13R, 13D (as applicable).

Includes M7900AAV.

Pressure Rating: 300 psig (2070 kPa).

Separation Chamber: Carbon steel body with threaded fitting for machined brass Air Scoop attachment. Powder coated Safety Red.

\*\* NOTE TO SPECIFIER \*\* Delete inlet and outlet size not required.

Inlet and Outlet Size:

2 inches (51 mm) Grooved ends.

2.5 inches (64 mm) Grooved ends.

3 inches (76 mm) Grooved ends.

4 inches (102 mm) Grooved ends.

6 inches (152 mm) Grooved ends.

1. inches (203 mm) Grooved ends. \*\* NOTE TO SPECIFIER \*\* Delete product not required.

Optional Water Collection Accessories:

Product: Model 7920AI. Water Collection Assembly with Audible Alarm.

Product: Model 7925VI. Water Collection Assembly with Visual Indicator.